**ultra high gloss by**

CARE & MAINTENANCE INSTRUCTIONS

WARNING Leave protective film in place until all other work on the project is completed.

MAINTENANCE TIPS For best results, use a damp soft cloth with mild soap and water. Absorb the excess water immediately with a clean and dry cloth.

AVOID

• The use of harsh or abrasive cleaners. The following cleaning agents should not be used under any circumstances: - Scouring and abrasive agents (abrasive powders, scouring pads, steel wool) - Polish, washing powder, furniture cleaner, bleach, wax - Steam cleaning equipment - Paint thinner or comparable product - Rubbing, denatured, or other alcohol-based solutions

• Heat sources directly applied to the surface.