****

**Care and Handling**:

\*“VISION” acrylic panels should be stored horizontally and should be well supported at all times.

\*Leave protective film in place until the project is complete.

\*Do not store panels outside.

 \*Avoid sliding the panels on the outer face surface to preserve the protection film.

**Protective Film**:

\*The surface of the “VISION” acrylic panels are covered with a protective film, which should stay on during processing and installation. After removal of the film, the surface is ready for daily use. No additional polishing is necessary.

\*“VISION” acrylic metallic colors have a directional design. Take note of the directional arrows on the protective film throughout machining and installation.

**Cleaning**:

\*Best results will be achieved using wet micro-fiber cloths or chamois with non-abrasive soap or detergent. Do not use brushes, scourers or scrapers at any time.

**Scratch Resistance**:

\*The “VISION” acrylic surfaces are scratch resistant, but not scratch proof. Please take precautions to protect the surface until the product has been installed.

**Machining**:

\*Machine “VISION” acrylic panels using high speed, very sharp carbine tools and moderate feed rates. “VISION” laminated panels may react to severe changes in humidity and temperature. A curvature of up to 2mm/1000mm may occur in some extreme environmental conditions.

**Installation**:

\*Adequate fixing should be provided at no greater than 500mm centers.

\*We recommend an air gap of 6mm adjacent to ovens and other heat sources.

\*When attaching decorative hardware be careful to not over tighten as this can distort the surface.

**Additional Feature**:

\*All “VISION” acrylic panels are dry-erase certified.